Kamil Káčer 211777









Normal mode:

Counting direction is always up overruns when passes the last bit

CTC mode

Allows greater controf of the compare match output frequency

PWM mode

In PWM mode counter is incremented until the counter value matches the top value. Counter is cleared in the next cycle.

Phase correct PWM mode

Counts until the counter value reatches top then it changes the counter direction

Main c.

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\*

\* Control LEDs using functions from GPIO and Timer libraries. Do not

\* use delay library any more.

\* ATmega328P (Arduino Uno), 16 MHz, AVR 8-bit Toolchain 3.6.2

\*

\* Copyright (c) 2018-2020 Tomas Fryza

\* Dept. of Radio Electronics, Brno University of Technology, Czechia

\* This work is licensed under the terms of the MIT license.

\*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

/\* Defines -----------------------------------------------------------\*/

#define LED\_D1 PB5

#define LED\_D2 PB4

#define LED\_D3 PB3

/\* Includes ----------------------------------------------------------\*/

#include <avr/io.h> // AVR device-specific IO definitions

#include <avr/interrupt.h> // Interrupts standard C library for AVR-GCC

#include "gpio.h" // GPIO library for AVR-GCC

#include "timer.h" // Timer library for AVR-GCC

/\* Function definitions ----------------------------------------------\*/

/\*\*

\* Main function where the program execution begins. Toggle three LEDs

\* on Multi-function shield with internal 8- and 16-bit timer modules.

\*/

int main(void)

{

/\* Configuration of three LEDs \*/

GPIO\_config\_output(&DDRB, LED\_D2);

GPIO\_write\_low(&PORTB, LED\_D2);

GPIO\_config\_output(&DDRB, LED\_D1);

GPIO\_write\_low(&PORTB, LED\_D1);

GPIO\_config\_output(&DDRB, LED\_D3);

GPIO\_write\_low(&PORTB, LED\_D3);

/\* Configuration of 8-bit Timer/Counter0 \*/

TIM0\_overflow\_16ms();

TIM0\_overflow\_interrupt\_enable();

/\* Configuration of 16-bit Timer/Counter1

\* Set prescaler and enable overflow interrupt \*/

TIM1\_overflow\_1s();

TIM1\_overflow\_interrupt\_enable();

/\* Configuration of 8-bit Timer/Counter2 \*/

TIM2\_overflow\_128us();

TIM2\_overflow\_interrupt\_enable();

// Enables interrupts by setting the global interrupt mask

sei();

// Infinite loop

while (1)

{

/\* Empty loop. All subsequent operations are performed exclusively

\* inside interrupt service routines ISRs \*/

}

// Will never reach this

return 0;

}

/\* Interrupt service routines ----------------------------------------\*/

/\*\*

\* ISR starts when Timer/Counter1 overflows. Toggle LEDs on

\* Multi-function shield. \*/

ISR(TIMER0\_OVF\_vect)

{

GPIO\_toggle(&PORTB, LED\_D1);

}

ISR(TIMER1\_OVF\_vect)

{

GPIO\_toggle(&PORTB, LED\_D2);

}

ISR(TIMER2\_OVF\_vect)

{

GPIO\_toggle(&PORTB, LED\_D3);

}

TIMER\_H

#ifndef TIMER\_H

#define TIMER\_H

/\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*

\*

\* Timer library for AVR-GCC.

\* ATmega328P (Arduino Uno), 16 MHz, AVR 8-bit Toolchain 3.6.2

\*

\* Copyright (c) 2019-2020 Tomas Fryza

\* Dept. of Radio Electronics, Brno University of Technology, Czechia

\* This work is licensed under the terms of the MIT license.

\*

\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*\*/

/\*\*

\* @file timer.h

\* @brief Timer library for AVR-GCC.

\*

\* @details

\* The library contains macros for controlling the timer modules.

\*

\* @note

\* Based on Microchip Atmel ATmega328P manual and no source file is

\* needed for the library.

\*

\* @copyright (c) 2019-2020 Tomas Fryza

\* Dept. of Radio Electronics, Brno University of Technology, Czechia

\* This work is licensed under the terms of the MIT license.

\*/

/\* Includes ----------------------------------------------------------\*/

#include <avr/io.h>

/\* Defines -----------------------------------------------------------\*/

/\*\*

\* @brief Defines prescaler CPU frequency values for Timer/Counter0.

\* @note F\_CPU = 16 MHz

\*/

#define TIM0\_stop() TCCR0B &= ~((1<<CS02) | (1<<CS01) | (1<<CS00));

#define TIM0\_overflow\_16us() TCCR0B &= ~((1<<CS2) | (1<<CS01)); TCCR0B |= (1<<CS00);

#define TIM0\_overflow\_128us() TCCR0B &= ~((1<<CS02) | (1<<CS00)); TCCR0B |= (1<<CS01);

#define TIM0\_overflow\_1ms() TCCR0B &= ~(1<<CS02); TCCR0B |= (1<<CS01) | (1<<CS00);

#define TIM0\_overflow\_4ms() TCCR0B &= ~((1<<CS01) | (1<<CS00)); TCCR0B |= (1<<CS02);

#define TIM0\_overflow\_16ms() TCCR0B &= ~(1<<CS01); TCCR0B |= (1<<CS02) | (1<<CS00);

/\*\*

\* @brief Defines prescaler CPU frequency values for Timer/Counter1.

\* @note F\_CPU = 16 MHz

\*/

#define TIM1\_stop() TCCR1B &= ~((1<<CS12) | (1<<CS11) | (1<<CS10));

#define TIM1\_overflow\_4ms() TCCR1B &= ~((1<<CS12) | (1<<CS11)); TCCR1B |= (1<<CS10);

#define TIM1\_overflow\_33ms() TCCR1B &= ~((1<<CS12) | (1<<CS10)); TCCR1B |= (1<<CS11);

#define TIM1\_overflow\_262ms() TCCR1B &= ~(1<<CS12); TCCR1B |= (1<<CS11) | (1<<CS10);

#define TIM1\_overflow\_1s() TCCR1B &= ~((1<<CS11) | (1<<CS10)); TCCR1B |= (1<<CS12);

#define TIM1\_overflow\_4s() TCCR1B &= ~(1<<CS11); TCCR1B |= (1<<CS12) | (1<<CS10);

/\*\*

\* @brief Defines prescaler CPU frequency values for Timer/Counter2.

\* @note F\_CPU = 16 MHz

\*/

#define TIM2\_stop() TCCR2B &= ~((1<<CS22) | (1<<CS21) | (1<<CS20));

#define TIM2\_overflow\_16us() TCCR2B &= ~((1<<CS22) | (1<<CS21)); TCCR2B |= (1<<CS20);

#define TIM2\_overflow\_128us() TCCR2B &= ~((1<<CS22) | (1<<CS20)); TCCR2B |= (1<<CS21);

#define TIM2\_overflow\_512us() TCCR2B &= ~(1<<CS22); TCCR2B |= (1<<CS21) | (1<<CS20);

#define TIM2\_overflow\_1024us() TCCR2B &= ~((1<<CS21) | (1<<CS20)); TCCR2B |= (1<<CS22);

#define TIM2\_overflow\_2048us() TCCR2B &= ~(1<<CS21); TCCR2B |= (1<<CS22) | (1<<CS20);

#define TIM2\_overflow\_4ms() TCCR2B &= ~(1<<CS20); TCCR2B |= (1<<CS22) | (1<<CS21);

#define TIM2\_overflow\_16ms() TCCR2B &= ((1<<CS22) | (1<<CS20) | (1<<C21));

/\*\*

\* @brief Defines interrupt enable/disable modes for Timer/Counter0.

\*/

#define TIM0\_overflow\_interrupt\_enable() TIMSK0 |= (1<<TOIE0);

#define TIM0\_overflow\_interrupt\_disable() TIMSK0 &= ~(1<<TOIE0);

/\*\*

\* @brief Defines interrupt enable/disable modes for Timer/Counter1.

\*/

#define TIM1\_overflow\_interrupt\_enable() TIMSK1 |= (1<<TOIE1);

#define TIM1\_overflow\_interrupt\_disable() TIMSK1 &= ~(1<<TOIE1);

/\*\*


\* @brief Defines interrupt enable/disable modes for Timer/Counter1.

\*/

#define TIM2\_overflow\_interrupt\_enable() TIMSK2 |= (1<<TOIE2);

#define TIM2\_overflow\_interrupt\_disable() TIMSK2 &= ~(1<<TOIE2);

#endif



Cannot see two other leds blinking because prescalar is still too small for human eye to recognize its change.